{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["NXXXXX"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"NXXXXX","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"merged":[[0,1,0,5]]}
[null,"Weight and Balance C-172 (NXXXXX)"]
[null,null,"Example. Not for flight planning use."]
[null,null,"Max GWT Takeoff (lb):",2550]
[null,null,"Max GWT Landing (lb):",2550]
[]
[null,"Item","Gallons","Weight (lb)","Arm (in)","Moment (lb-in)"]
[null,"Aircraft Empty Weight",null,1646.1,{"v":40.16779,"d":"40.2"},{"$f":"PRODUCT(D7:E7)","v":{"v":66120.199119,"d":"66120.2"}}]
[null,"Front Seats",null,360,{"v":37,"d":"37.0"},{"$f":"D8*E8","v":13320}]
[null,"Rear Seats",null,0,{"v":73,"d":"73.0"},0]
[null,"Baggage 1 (120 lbs. Max.)",null,10,{"v":95,"d":"95.0"},950]
[null,"Baggage 2 (50 lbs. Max.)",null,0,{"v":123,"d":"123.0"},0]
[null,"Fuel (53 Gallons Max)",53,{"$f":"6.02*C12","v":{"v":319.06,"d":"319"}},{"v":48,"d":"48.0"},{"v":15314.880000000001,"d":"15315"}]
[null,"Fuel used taxi",1,{"$f":"6.02*C13","v":{"v":6.02,"d":"6"}},{"v":48,"d":"48.0"},{"v":288.96,"d":"289"}]
[null,"Takeoff Condition",null,{"$f":"SUM(D7:D12)-D13","v":{"v":2329.14,"d":"2329"}},null,{"$f":"SUM(F7:F12)-F13","v":{"v":95416.119119,"d":"95416"}}]
[{"$nulls":3},"Takeoff CG (in):",{"$f":"F14/D14","v":{"v":40.9662446735705,"d":"41.0"}}]
[]
[]
[null,"Fuel used in Cruise",30,{"$f":"6.02*C18","v":{"v":180.6,"d":"181"}},{"v":48,"d":"48.0"},{"$f":"D18*E18","v":{"v":8668.8,"d":"8669"}}]
[null,"Landing Weight",null,{"$f":"D14-D18","v":{"v":2148.54,"d":"2149"}},null,{"$f":"F14-F18","v":{"v":86747.31911899999,"d":"86747"}}]
[{"$nulls":3},"Landing CG (in):",{"$f":"F19/D19","v":{"v":40.375007735020056,"d":"40.4"}}]
{"$rows_empty":38}
["Weight and Balance Calculation Guide",{"$nulls":3}," © 2019-2024 Flex Air Flight School"]